**Speakerphone Paging codes**

* **Speakerphone Page:**

Access code for transmitting a message to multiple phones via their loudspeakers

(ex. Dial '\*399' to speakerphone all Extensions defined under Enhanced Services)

* **Single Speakerphone Page:**

Access code for transmitting a message to phones loudspeaker

(ex. Dial '\*400 + $EXTENSION' to transmit a message to provided extension/phone loudspeaker)

PBXware 3.8 brings in new feature in form of Two Way Speakerphone Paging. In order to start two way communication with preferred extension on the system dial \*400 + \* + $EXTENSION. For example, if you would like to initiate two way speakerphone paging with extension 1038 you will dial: \*400\*1038.

* **Two Way Speakerphone Page:**

Access code used to start a two way communication through phones loudspeaker

(ex. Dial '\*400 + \* + $EXTENSION' to start communication to provided extension/phone loudspeaker)